			2011-10-18
1,use jungo usb2serail driver
2,add google VID for surpport window fastboot.

			2011-11-29
1,use new tether.inf for RNDIS driver, fix the potential RNDIS problem on some windows os's
			
			2012-02-11
1,add the mocor usb2serial drivers PID
2,fix the envisiment variable "MaxTransferSize"(in sprd_enum.inf) from 0x2000 to default 0x200, for in factory,
  some PC driver cannot work for allocating memory fail...
